**Learning Module Number 9**

**Design by the Direct Analysis Method**

**Overview**

The design of a portal frame is investigated for two options available within the Direct Analysis Method as defined in Chapter C of the AISC *Specification for Structural Steel Buildings* (2022). Rigorous second-order analyses are employed to check the adequacy of compact doubly symmetric members subject to flexure and axial force.

**Learning Objectives**

* Apply the Direct Analysis Method of design to assess the adequacy of a structural system.
* Employ rigorous second-order analyses to determine required strengths in beam-columns.
* Utilize notional loads in place of both direct modeling of initial imperfections and stiffness reduction due to partial yielding.
* Use an interaction equation to check the adequacy of members subject to the combination of flexure and axial force.
* Use the ratio of second- to first-order drifts as an indicator of a system’s sensitivity to second-order effects.

**Method**

Begin by preparing two identical computational models of the portal frame shown in Fig. 1; one of these models will be modified and used in Case Studies 1 and 2, and the other model will be used in Case Study 3. The columns are W12x58 (A992) of length 12’-0” and oriented for minor-axis bending, and the beam is a W24x76 (A992) that is fully braced out-of-plane. Different values of *Qu* will be used in the below studies, and in all analyses, stiffness reduction shall be included by reducing *E* by a factor of 0.8. Initial member imperfections (out-of-straightness) need not be modeled. Begin by completing Table A.



Figure 1.

Case studies:

1. Modify one of the models to include the effects of initial construction tolerance imperfections by assuming an out-of-plumbness ratio of H/500, where H is the story height. With *Qu* = 100 kips, perform a second-order analysis that includes an additional stiffness reduction factor 0.8*b* per Section C.2.3 of the AISC *Specification for Structural Steel Buildings* (2022). Complete Table 1 using the analysis results and the information calculated in Table A.
2. Employing the same model and analysis parameters used in above study, determine the maximum value for *Qu* that will satisfy the AISC interaction equation (Eq. H1-1a,b). This may take several trial and error iterations. Complete Table 2 for the analysis results that correspond to your maximum value of *Qu*.
3. Using the second computational model (i.e., the one that has not been modified to include imperfections), perform a second-order elastic analysis with *Qu* = 100 kips and a lateral load equaling the sum of 0.1*Qu* and potentially two notional loads. The notional load of 0.002*Qu* represents the out-of-plumb imperfection, and the notional load 0.001*Qu* (if required) represents the additional stiffness reduction previously modeled by the *b* factor. Complete Table 4 using the analysis results and information calculated in Table 1.

Table A. Applicable to all cases.

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Member | *K* | *L* (in.) | Section | Axis | *r* (in.) | *Ag* (in.2) | *Z* (in.3) | *cPn* | *bMn* |
| Left Column | 1.0 | 144 | W12x58 | minor |  |  |  |  |  |
| Right Column | 1.0 | 144 | W12x58 | minor |  |  |  |  |  |
| Beam | 1.0 | 240 | W24x76 | major |  |  |  |  |  |

Table 1.

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 1. Direct Analysis Method with imperfections modeled and *b* included in analysis | | | | | | 0.8 *E* = ksi | |
| Gravity Load  *Qu* = 100 kips | Lateral Load  0.1*Qu* = 10 kips | Model includes lateral imperfection of  H/500 = in. | | | Additional stiffness reduction modeled by use of *b* included in the analysis | | |
| Member | *Pu* (kips) | *cPn* (kips) | *M*u (kip-in) | *bMn* (kip-in) | | AISC Eq. H1-1a/b | OK/NG? |
| Left Column |  |  |  |  | |  |  |
| Right Column |  |  |  |  | |  |  |
| Beam |  |  |  |  | |  |  |

Table 2.

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 2. Direct Analysis Method with imperfections modeled and *b* included in analysis | | | | | | 0.8 *E* = ksi | |
| Gravity Load  *Qu* = kips | Lateral Load  0.1*Qu* = kips | Model includes lateral imperfection of  H/500 = in. | | | Additional stiffness reduction modeled by use of *b* included in the analysis | | |
| Member | *Pu* (kips) | *cPn* (kips) | *M*u (kip-in) | *bMn* (kip-in) | | AISC Eq. H1-1a/b | OK/NG? |
| Left Column |  |  |  |  | |  | OK |
| Right Column |  |  |  |  | |  | OK |
| Beam |  |  |  |  | |  | OK |

Table 3.

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 3. Direct Analysis Method with notional loads and no imperfections or *b* included | | | | | | 0.8 E = ksi | | |
| Gravity Load  *Qu* = 100 kips | Lateral Load  0.1*Qu* = 10 kips | Imperfection Notional Load  0.002*Qu* = kips | | Stiffness Notional Load  0.001*Qu* = kips | | | Total Lateral Load  = kips | |
| Member | *Pu* (kips) | *cPn* (kips) | *M*u (kip-in) | | *bMn* (kip-in) | AISC Eq. H1-1a/b | | OK/NG? |
| Left Column |  |  |  | |  |  | |  |
| Right Column |  |  |  | |  |  | |  |
| Beam |  |  |  | |  |  | |  |

Hints:

1. Suggested units are kips, inches, and ksi.
2. Do not include the self-weight of the members.

**MASTAN2 Details**

The following suggestions are for those employing MASTAN2 to calculate the above computational strengths:

* Subdivide the members into 4 elements.
* By default, MASTAN2 aligns the web (local y-axis) in the global X-Y plane. Use the *Re-orient Element(s)* option to rotate the member 90 degrees to investigate minor-axis bending of the columns.
* Initial imperfections (as needed) can be included by either extensive use of the *Move Node* option, or much more easily by “permanently bending” the frame through the combined use of a lateral load analysis and MASTAN2’s post-processing option *Results*-*Update Geometry*.
* For Cases 1 and 2, employ second-order inelastic analyses[[1]](#footnote-1) with:
  + - Planar frame analysis type
    - Predictor-corrector solution scheme
    - Load increment size of 0.05
    - Maximum number of increments set to 100
    - Maximum applied load ratio set to 1.0
    - Modulus set to *Et* (not *Etm*; *Et* employ’s AISC’s stiffness reduction *b* factor)
* For Case 3, employ a second-order elastic analyses with:
  + - Planar frame analysis type
    - Predictor-corrector solution scheme
    - Load increment size of 0.05
    - Maximum number of increments set to 100
    - Maximum applied load ratio set to 1.0
* For Question 4 (below), employ a second-order inelastic analysis with:
  + - Planar frame analysis type
    - Predictor-corrector solution scheme
    - Load increment size of 0.05
    - Maximum number of increments set to 100
    - Maximum applied load ratio set to 5.0
    - Modulus set to *Etm* (MASTAN2’s approximation for partial yielding/residual stresses)
* For Question 3 (below), prepare force-displacement curves using MASTAN2’s MSAPlot feature.

**Questions**

1. Based on the results presented in Tables 1 and 3, what can you conclude about the two variations of the Direct Analysis Method? Include in your response the pros and cons of each variation.
2. For this system and based on the results recorded in Tables 1 and 2, what was the minimum value of the stiffness reduction factor *b* employed in the analysis? Please interpret this number.
3. For the Case Study 1 computation model with *Qu* = 100 kips, perform first- and second-order elastic analyses. Prepare a single plot that includes two curves (one for each analysis) with lateral deflection at the upper left corner of the frame as the abscissa and applied load *Qu* as the ordinate. Record the maximum lateral deflection for each analysis.
   1. Based on the ratio of these second- to first-order drifts, what can you conclude about this system’s sensitivity to second-order effects? Does the plot support your conclusion?
   2. If the first-order moment at one end of the beam was 1000 kip-in, use the above ratio to estimate this moment if equilibrium is formulated on the actual deformed shape of the system (i.e. based on an analysis that includes second-order effects)? Confirm your estimate by comparing actual moments taken from first- and second-order analyses of the system.
   3. Given that the beam resists a relatively small amount of axial force, explain why second-order effects are so significant in this member? In general beam design, when can second-order effects be neglected and when must they be included?
4. What does a second-order inelastic analysis for Case Study 2 show? Per Appendix 1 of the AISC *Specification for Structural Steel Buildings* (2022), be sure to reduce the yield strength of the steel to 45 ksi and redefine *E* to 0.9 x 29000 ksi. Describe the frame’s limit state behavior, including locations of yielding and maximum applied load ratio. Discuss these findings in relation to the data obtained in Table 2.

**More Fun with Computational Analysis!**

1. Repeat the above exercise with the column bases rigidly attached to the foundations.
2. Repeat the above exercise with the same beam size, but with HSS10x10x1/2 (A500Gr.B) columns.
3. Include additional case studies that are based on the effective length and first-order analysis design methods defined in Appendix 7 of the AISC *Specification for Structural Steel Buildings* (2022).

**Additional Resources**

MS Excel spreadsheet: *9\_DirectAnalysisMethod.xlsx*

MASTAN2 – LM9 Tutorial Video [12 min]:

<http://www.youtube.com/watch?v=Poda7uKXAJQ>

MASTAN2 - How to re-orient elements for minor-axis bending [2 min]:

<http://www.youtube.com/watch?v=kqcPlDvw95U>

MASTAN2 - How to include an initial frame sway imperfection (out-of-plumb of H/500) [7 min]:

<http://www.youtube.com/watch?v=OTL3sx4W9TM>

MASTAN2 - How to account for partial yielding accentuated by residual stresses [1 min]:

<http://www.youtube.com/watch?v=m8ZXM02Cbu4>

MASTAN2 - How to plot response curves with MSAPlot [3 min]:

<http://www.youtube.com/watch?v=vS67MT0M1PQ>

AISC *Specification for Structural Steel Buildings and Commentary* (2022):

<https://www.aisc.org/publications/steel-standards/aisc-360/>

MASTAN2 software:

<http://www.mastan2.com/>

1. Although the Direct Analysis Method is based on second-order elastic analysis, MASTAN2 only provides access to the stiffness reduction *b* factor in its second-order inelastic analysis feature. [↑](#footnote-ref-1)